|  |  |  |  |
| --- | --- | --- | --- |
| **Specifications A7AQ26** | | | |
| Model | Shuangye 26 inch e bike A7AQ26 | Wheel | 26 inch wheel |
| Color | White/Dark Blue/Black | Tyre | 26”\*4.0 fat tire |
| Motor | Shuangye 36v/48v 250W/350W/500W brushless motor | Gear | Shman 7 Speed |
| Battery | 36V10AH/12AH 48V15AH  Lithium battery | PAS | Five adjustable speed 1:1 pedal assistant |
| Range | 1:1 PAS mode, 40-60KM | Chain | Rust resistant chain |
| Warranty | motor & battery 1 years | Handle bar | Aluminum alloy |
| Charger | AC100V-240V,42V 2A | crankset | Aluminum alloy |
| Charging time | 5-7 hours | Saddle | Comfortable Saddle |
| Max speed | 25km/h 30km/h 35km/h based on flat road without wind | Display | LCD Display |
| Loading | 200KG | headlight | 1 W LED headlight |
| Frame | Aluminum Alloy frame | sticker &color | Shuangye(can OEM) |
| Wheel rim | Aluminum alloy | Pedal | aluminum |
| Front fork | suspension aluminum fork | Certification | CE EN15194 |
| Front brake | 160 disc brake | Weight | N.W: 28kgs G.W:35kgs |
| Rear brake | 160 disc brake | Carton size | 149\*39\*80CM |
| Motor Effect | ≥80% | 20'GP container | 50PCS(5.69\*2.13\*2.18) |
| port | zhuhai or zhenzhen | MOQ | 10 pcs |

An fat electric bike with a powerful 250/350/500 watt motor, ample 36/48 volt battery and shimano 7 speed drivetrain

Comfortable saddle, ergonomic grips and full suspension fork with lockout, two color and two frame size 26" for choices

Integrated headlight, front and rear 160 disc brakes, fat electric bike is 26\*4.0 fat tires and two drive modes (throttle and pedal assist)

No quick release on the wheels, battery has to be powered on independently from the LCD display, have bottle cage or rack bosses but there are optional fenders available