|  |
| --- |
| **Specifications A5AH26** |
| Model | A5AH26 | Wheel | 26 inch wheel |
| Color | Dark blue/Yellow/White | Tyre | 26"\*1.95 |
| Motor | Shuangye 36v 250w brushless motor | Gear | 21 speed shimano  |
| Initiating mode | PAS | PAS | Five adjustable speed 1:1 pedal assistant  |
| Battery | 36V 9Ah Lithium-ion battery hide in the frame | Chain | Rust resistant chain |
| Range | 1:1 PAS mode, 40-60km | Handle bar | Aluminum alloy |
| Warranty | Motor & battery 1 year | Crankset | Aluminum alloy |
| Charger | AC100V-240V,42V 2A | Saddle | Mountain bike saddle |
| Charging time | 4-7h | Display | 5 inch LCD3 displayer |
| Max speed | 25Km/h | Front light | 3W LED |
| Loading | 120Kg | Mudguard | Steel |
| Frame | 6061 Aluminum frame | Handlebar | Aluminum alloy |
| Wheel rim | Aluminum alloy | Sticker &color | Shuangye(can OEM) |
| Front fork | Aluminuim alloy suspension | Pedal | Aluminum alloy |
| Front brake | Tektro 160 disc brake | Certification | CE TUV |
| Rear brake | Tektro 160 disc brake | Weight | GW: 29.3Kg NT:20.8Kg |
| Climbing ability | ≥12° | Carton size | 138CM\*79CM\*29CM |